
ReadMe



InterruptIn Start(D9);//start button

InterruptIn Stop(D8);//stop button

AnalogIn Ain(A0);

AnalogOut Aout(PA\_4); //D7

uLCD\_4DGL uLCD(D1,D0,D2);//like previous lab

After implemented, press start button, after 1 sec, run FFTHW\_2.py, and press stop button. You can get a figure.